Figure 15. The average energy received of each sensor node with sensor nodes increasing from 25 to 125